Hauptseite | Klassenhierarchie | Alphabetische Liste | Auflistung der Klassen | Auflistung der Dateien | Klassen-Elemente

# Cfps Elementverzeichnis

Vollständige Aufstellung aller Elemente für Cfps einschließlich aller geerbten Elemente.

AddTrace(const char *lpszMsg, CTraceObject::eTraceLevel eLevel=CTraceObject::MT_ERROR) | CTraceObject | `[virtual]`
AddTrace(std::ostrstream &oStream, CTraceObject::eTraceLevel eLevel=CTraceObject::MT_ERROR) | CTraceObject |
Cfps() | Cfps |
Cfps(const Cfps &NewObject) | Cfps | `[private]`
ConnectIndication(void) | Cfps | `[private, virtual]`
ConnectRequest(void) | CTCPIPComm |
CTCPIPCommConnect::ConnectRequest(SOCKET PassiveSocket) | CTCPIPCommConnect |
CONVERT_TO enum Bezeichner | Cfps |
ConvTCPAddrToSocketAddr(const short TCPport, const char *pIPAddr) | CTCPIPCommConnect |
ConvToInAddr(unsigned long nIPAddress) const | CTCPIPCommConnect |
CTCPIPComm(const short TCPport, const char *pIPAddress, const bool PassiveConnection, const long MaxSendDataLen, const long MaxRecvDataLen) | CTCPIPComm |
CTCPIPComm(void) | CTCPIPComm | `[protected]`
CTCPIPCommConnect() | CTCPIPCommConnect |
CTCPIPCommReceive(const long MaxRecvBufferLen=8192) | CTCPIPCommReceive |
CTCPIPCommSend(const long MaxSendBufferLen=8192) | CTCPIPCommSend |
CTCPIPConnector() | CTCPIPConnector |
CTraceObject() | CTraceObject |
DisconnectIndication(void) | Cfps | `[private, virtual]`
DisconnectRequest(void) | CTCPIPCommConnect |
eTraceLevel enum Bezeichner | CTraceObject |
FetchData(RECEIVED_TYPE &Command, ADDRESS_TYPE &nAddress, unsigned int &uiLength, std::vector< unsigned char > &aucData) | Cfps |
FetchStuetzArrayFromFps(void) | Cfps |
GetBasePort(void) const | Cfps |
GetCallnumber(char *pcCallnumber, unsigned int ucBufLen) | Cfps |
GetCallNumber(char *pcCallNumber, unsigned int uiBufLen) | Cfps |
GetCOMPort(void) const | CTCPIPConnector | `[inline]`
GetCurrentConnectionType(void) const | Cfps |
GetCurrentSensorValue(float &CurSen, CONVERT_TO eConvertTo=SPEC) | Cfps |
GetCurrentTemperature(float &CurrentTemperature) | Cfps |
GetCurrentVoltage(float &CurOperatingVoltage) | Cfps |
GetIsTraceLevelAktivated(CTraceObject::eTraceLevel eLevel) const | CTraceObject | `[protected]`
GetLastErrorText(DWORD dwError) (Definiert in CTraceObject) | CTraceObject | `[static]`
GetLastSocketError(void) const | CTCPIPComm | `[inline]`
GetMaxBlockLength(void) const | Cfps | `[private]`
GetMaxRetryCount(void) const | Cfps | `[private]`
GetModemConnectString(char *pcModemConnectString, unsigned int BufLen) | Cfps |
GetModemDialString(char *pcModemDialString, unsigned int BufLen) | Cfps |
GetModemDialTimeout(void) const | Cfps |
GetModemInitString(char *pcModemInitString, unsigned int BufLen) | Cfps |
GetModemInitTimeout(void) const | Cfps |
GetModemOkString(char *pcModemOkString, unsigned int BufLen) | Cfps |
GetOperatingState(int &Flags) | Cfps |
GetOutOfRangeFlags(int &Flags) | Cfps |
GetPortB(int &Flags) | Cfps |
GetPortBSamples(int PortBSample[640], unsigned int uiBegin=0, unsigned int uiLength=640) | Cfps |
GetRcvTimeOut(void) const | Cfps |
GetRemoteAddr(void) | CTCPIPCommConnect | `[inline]`
GetRemoteIPAddr(void) | CTCPIPCommConnect | `[inline]`
GetSensorSamples(float SenSamp[640], unsigned int uiBegin=0, unsigned int uiLength=640) | Cfps |
GetServiceInfo(int &Week, int &Year, int &Serialnumber) | Cfps |
GetSocket(void) | CTCPIPCommConnect | `[inline]`
GetTcpIpAddress(char *pcIpAddress, SIZE_T BufLen) | Cfps |
GetTcpIpPort(void) | Cfps |
GetTolerance(float &fUnterTolerance, float &fUeberTolerance) | Cfps |
GetUseCrcCheck(void) const | CTCPIPConnector | `[protected]`
GetVoltageSamples(float VoltageSample[640], unsigned int uiBegin=0, unsigned int uiLength=640) | Cfps |
InformAboutNewData(const HANDLE hEvent) const | Cfps | `[private]`
Initialize(const short TCPport, const char *pIPAddress, const bool PassiveConnection, const long MaxSendDataLen, const long MaxRecvDataLen) | CTCPIPComm | `[protected]`
CTCPIPCommReceive::Initialize(const SOCKET Socket) | CTCPIPCommReceive |
CTCPIPCommSend::Initialize(const SOCKET Socket) | CTCPIPCommSend |
CTCPIPCommConnect::Initialize(const short TCPport, const char *pIPAddress, const bool PassiveConnection=false) | CTCPIPCommConnect |
initialize(void) | Cfps | `[virtual]`
CTCPIPConnector::initialize(const short TCPport, const char *pIPAddress) | CTCPIPConnector | `[virtual]`
CTCPIPCommReceive::InitializeClass(const long MaxRecvBufferLen) | CTCPIPCommReceive | `[protected]`
CTCPIPCommSend::InitializeClass(const long MaxSendBufferLen) | CTCPIPCommSend | `[protected]`
InitModem(void) | Cfps |
IsConnected(void) const | CTCPIPConnector |
IsSamplingDone(bool &bDone) | Cfps |
Loc_GetRcvData(RECEIVED_TYPE eExpectedRcvType, ADDRESS_TYPE nAddress, unsigned int uiLength, std::vector< unsigned char > &aucBuffer) | Cfps | `[private]`
LockFpsReq(void) | Cfps | `[private]`
m_aucEeprom | Cfps | `[private]`
m_aucProgram | Cfps | `[private]`
m_aucRam | Cfps | `[private]`
m_bRcvRawData (Definiert in CTCPIPConnector) | CTCPIPConnector | `[protected]`
m_bRcvRawDataFinished (Definiert in CTCPIPConnector) | CTCPIPConnector | `[protected]`
m_dwRcvTimeOut | Cfps | `[private]`
m_eNeuVerb | Cfps | `[private]`
m_hBlockRequest | Cfps | `[private]`
m_hRcvEventConnect | Cfps | `[private]`
m_hRcvEventDisconnect | Cfps | `[private]`
m_hRcvEventFpsDataMovement | Cfps | `[private]`
m_oConvert | Cfps |
m_oRcvBuffer | Cfps | `[private]`
m_sCallNumber | Cfps | `[private]`
m_sModemConnectString | Cfps | `[private]`
m_sModemDialString | Cfps | `[private]`
m_sModemInitString | Cfps | `[private]`
m_sModemOkString | Cfps | `[private]`
m_sRcvRawDataString (Definiert in CTCPIPConnector) | CTCPIPConnector | `[protected]`
m_sTcpIpAddress | Cfps | `[private]`
m_uiBasePort | Cfps | `[private]`
m_uiMaxBlockLength | Cfps | `[private]`
m_uiMaxRetry | Cfps | `[private]`
m_uiModemDailTimeout | Cfps | `[private]`
m_uiModemInitTimeout | Cfps | `[private]`
m_uiTcpIpPort | Cfps | `[private]`
MM enum Wert | Cfps |
MODEM enum Wert (Definiert in Cfps) | Cfps |
MT_DEBUG enum Wert (Definiert in CTraceObject) | CTraceObject |
MT_ERROR enum Wert (Definiert in CTraceObject) | CTraceObject |
MT_INFO enum Wert (Definiert in CTraceObject) | CTraceObject |
MT_WARNING enum Wert (Definiert in CTraceObject) | CTraceObject |
MV enum Wert | Cfps |
NETZWERK enum Wert | Cfps |
operator=(const Cfps &OldObject) | Cfps | `[private]`
PasswordLogin(char *szIpAddress, char *szPassword, unsigned int uiBasePort, unsigned int uiPortnumber) | Cfps |
ReadDataPointHeader(void) | Cfps | `[private]`
ReadDataPoints(void) | Cfps | `[private]`
ReadEepromData(ADDRESS_TYPE nAddress, unsigned int uiLength) | CTCPIPConnector |
ReadEepromDataCnf(ADDRESS_TYPE nAddress, unsigned int uiLength, const std::vector< unsigned char > &aucData) | Cfps | `[private, virtual]`
ReadEepromDataReq(ADDRESS_TYPE nAddress, unsigned int uiLength) | Cfps | `[private, virtual]`
ReadFpsEeprom(ADDRESS_TYPE nAddress, unsigned int uiLength) | Cfps | `[protected]`
ReadFpsProgram(ADDRESS_TYPE nAddress, unsigned int uiLength) | Cfps | `[protected]`
ReadFpsRam(ADDRESS_TYPE nAddress, unsigned int uiLength) | Cfps | `[protected]`
ReadInterpolatedSensor(SENSOR_TYPE &CurrentSensorValues) | Cfps |
ReadProfileFile(const std::string &sFilename) | Cfps |
ReadProfileFileConnectionType(const std::string &sFilename) | Cfps |
ReadProgramData(ADDRESS_TYPE nAddress, unsigned int uiLength) | CTCPIPConnector |
ReadProgramDataCnf(ADDRESS_TYPE nAddress, unsigned int uiLength, const std::vector< unsigned char > &aucData) | Cfps | `[private, virtual]`
ReadProgramDataReq(ADDRESS_TYPE nAddress, unsigned int uiLength) | Cfps | `[private, virtual]`
ReadRamData(ADDRESS_TYPE nAddress, unsigned int uiLength) | CTCPIPConnector |
ReadRamDataCnf(ADDRESS_TYPE nAddress, unsigned int uiLength, const std::vector< unsigned char > &aucData) | Cfps | `[private, virtual]`
ReadRamDataReq(ADDRESS_TYPE nAddress, unsigned int uiLength) | Cfps | `[private, virtual]`
ReadSensor(SENSOR_TYPE &CurrentSensorValues) | Cfps |
Receive(void *pData, long DataLen) | CTCPIPConnector | `[protected, virtual]`
ResetEx(void) | Cfps |
RS232 enum Wert | Cfps |
SaveTolerance(float fUnterTolerance, float fUeberTolerance) | Cfps |
Send(const void *pData, const long DataLen) | CTCPIPComm |
SendReadEepromDataCnf(ADDRESS_TYPE nAddress, const std::vector< unsigned char > &aucData) | CTCPIPConnector |
SendReadProgramDataCnf(ADDRESS_TYPE nAddress, const std::vector< unsigned char > &aucData) | CTCPIPConnector |
SendReadRamDataCnf(ADDRESS_TYPE nAddress, const std::vector< unsigned char > &aucData) | CTCPIPConnector |
SendStatusInfo(ADDRESS_TYPE nAddress, unsigned int uiLength, std::vector< unsigned char > aucData) | CTCPIPConnector |
SendWriteEepromDataCnf(ADDRESS_TYPE nAddress, unsigned int uiLength) | CTCPIPConnector |
SendWriteProgramDataCnf(ADDRESS_TYPE nAddress, unsigned int uiLength) | CTCPIPConnector |
SendWriteRamDataCnf(ADDRESS_TYPE nAddress, unsigned int uiLength) | CTCPIPConnector |
SetBasePort(const unsigned int nBasePort) | Cfps |
SetCallNumber(char *pcNewCallNumber) | Cfps |
SetCallnumber(char *pcNewCallnumber) | Cfps |
SetCOMPort(CCOMConnector *pMsg) | CTCPIPConnector | `[inline]`
SetCurrentConnectionType(const VERBINDUNG eNewConnectionType) | Cfps |
SetMaxBlockLength(unsigned int uiNewMaxBlockLength) | Cfps | `[private]`
SetMaxRetryCount(const unsigned int uiNewRetryCount) | Cfps | `[private]`
SetModemConnectString(char *pcModemConnectString) | Cfps |
SetModemDialString(char *pcNewModemDialString) | Cfps |
SetModemDialTimeout(const unsigned int uiNewTimeoutValue) | Cfps |
SetModemInitString(char *pcNewModemInitString) | Cfps |
SetModemInitTimeout(const unsigned int uiNewTimeOut) | Cfps |
SetModemOkString(char *pcModemOkString) | Cfps |
SetOperatingState(int Flags) | Cfps |
SetRcvTimeOut(const DWORD dwNewTimeOut) | Cfps |
SetTcpIpAddress(char const *pcIpAddress) | Cfps |
SetTcpIpPort(unsigned int uiNewPort) | Cfps |
SetTraceLevel(int nTraceLevelMask) | CTraceObject |
SetUseCrcCheck(const bool bUseCrc) | CTCPIPConnector | `[protected]`
SPEC enum Wert (Definiert in Cfps) | Cfps |
StartReceiving(void) | CTCPIPCommReceive |
StartSampling(void) | Cfps |
StatusInfo(ADDRESS_TYPE nAddress, unsigned int uiLength, const std::vector< unsigned char > &aucData) | Cfps | `[private, virtual]`
StoreData(const RECEIVED_TYPE Command, const ADDRESS_TYPE nAddress, const unsigned int uiLength, const std::vector< unsigned char > &aucData=std::vector< unsigned char >::vector()) | Cfps |
StoreStuetzArrayInFps(void) | Cfps |
terminate(void) | CTCPIPConnector |
CTCPIPCommReceive::Terminating(void) const | CTCPIPCommReceive | `[inline]`
CTCPIPCommReceive::Terminating(bool Terminating) | CTCPIPCommReceive | `[inline]`
CTCPIPCommSend::Terminating(void) const | CTCPIPCommSend | `[inline]`
CTCPIPCommSend::Terminating(bool Terminating) | CTCPIPCommSend | `[inline]`
CTCPIPCommConnect::Terminating(void) const | CTCPIPCommConnect | `[inline]`
TestRcvData(RECEIVED_TYPE Command, ADDRESS_TYPE nAddress, unsigned int uiLength, std::vector< unsigned char > &aucTestedData) | Cfps | `[private]`
UnlockFpsReq(void) | Cfps | `[private]`
VERBINDUNG enum Bezeichner | Cfps |
WaitForData(void) | Cfps | `[protected]`
WriteDataPointHeader(void) | Cfps | `[private]`
WriteDataPoints(void) | Cfps | `[private]`
WriteEepromData(ADDRESS_TYPE nAddress, const std::vector< unsigned char > &aucData) | CTCPIPConnector |
WriteEepromDataCnf(ADDRESS_TYPE nAddress, unsigned int uiLength) | Cfps | `[private, virtual]`
WriteEepromDataReq(ADDRESS_TYPE nAddress, unsigned int uiLength, const std::vector< unsigned char > &aucData) | Cfps | `[private, virtual]`
WriteFpsEeprom(ADDRESS_TYPE nAddress, unsigned int uiLength, std::vector< unsigned char > aucData) | Cfps | `[protected]`
WriteFpsProgram(ADDRESS_TYPE nAddress, unsigned int uiLength, std::vector< unsigned char > aucData) | Cfps | `[protected]`
WriteFpsRam(ADDRESS_TYPE nAddress, unsigned int uiLength, std::vector< unsigned char > aucData) | Cfps | `[protected]`
WriteProfileFile(std::string sFilename) | Cfps |
WriteProgramData(ADDRESS_TYPE nAddress, const std::vector< unsigned char > &aucData) | CTCPIPConnector |
WriteProgramDataCnf(ADDRESS_TYPE nAddress, unsigned int uiLength) | Cfps | `[private, virtual]`
WriteProgramDataReq(ADDRESS_TYPE nAddress, unsigned int uiLength, const std::vector< unsigned char > &aucData) | Cfps | `[private, virtual]`
WriteRamData(ADDRESS_TYPE nAddress, const std::vector< unsigned char > &aucData) | CTCPIPConnector |
WriteRamDataCnf(ADDRESS_TYPE nAddress, unsigned int uiLength) | Cfps | `[private, virtual]`
WriteRamDataReq(ADDRESS_TYPE nAddress, unsigned int uiLength, const std::vector< unsigned char > &aucData) | Cfps | `[private, virtual]`
WriteSensor(SENSOR_TYPE NewSensorValues) | Cfps |
~Cfps() | Cfps | `[virtual]`
~CTCPIPComm() | CTCPIPComm | `[virtual]`
~CTCPIPCommConnect() | CTCPIPCommConnect | `[virtual]`
~CTCPIPCommReceive() | CTCPIPCommReceive | `[virtual]`
~CTCPIPCommSend() | CTCPIPCommSend | `[virtual]`
~CTCPIPConnector() | CTCPIPConnector | `[virtual]`
~CTraceObject() | CTraceObject | `[virtual]`