Hauptseite | Klassenhierarchie | Alphabetische Liste | Auflistung der Klassen | Auflistung der Dateien | Klassen-Elemente | Datei-Elemente

# Cfps Elementverzeichnis

Vollständige Aufstellung aller Elemente für Cfps einschließlich aller geerbten Elemente.

Cfps() | Cfps |
CONVERT_TO enum Bezeichner | Cfps |
CTCPIPConnector() | CTCPIPConnector |
FetchData(RECEIVED_TYPE &Command, ADDRESS_TYPE &nAddress, unsigned int &uiLength, std::vector< unsigned char > &aucData) | Cfps |
FetchStuetzArrayFromFps(void) | Cfps |
GetBasePort(void) const | Cfps |
GetCallnumber(char *pcCallnumber, unsigned int ucBufLen) | Cfps |
GetCallNumber(char *pcCallNumber, unsigned int uiBufLen) | Cfps |
GetCOMPort(void) const | CTCPIPConnector | `[inline]`
GetCurrentConnectionType(void) const | Cfps |
GetCurrentSensorValue(float &CurSen, CONVERT_TO eConvertTo=SPEC) | Cfps |
GetCurrentTemperature(float &CurrentTemperature) | Cfps |
GetCurrentVoltage(float &CurOperatingVoltage) | Cfps |
GetModemConnectString(char *pcModemConnectString, unsigned int BufLen) | Cfps |
GetModemDialString(char *pcModemDialString, unsigned int BufLen) | Cfps |
GetModemDialTimeout(void) const | Cfps |
GetModemInitString(char *pcModemInitString, unsigned int BufLen) | Cfps |
GetModemInitTimeout(void) const | Cfps |
GetModemOkString(char *pcModemOkString, unsigned int BufLen) | Cfps |
GetOperatingState(int &Flags) | Cfps |
GetOutOfRangeFlags(int &Flags) | Cfps |
GetPortB(int &Flags) | Cfps |
GetPortBSamples(int PortBSample[640], unsigned int uiBegin=0, unsigned int uiLength=640) | Cfps |
GetRcvTimeOut(void) const | Cfps |
GetSensorSamples(float SenSamp[640], unsigned int uiBegin=0, unsigned int uiLength=640) | Cfps |
GetServiceInfo(int &Week, int &Year, int &Serialnumber) | Cfps |
GetTcpIpAddress(char *pcIpAddress, SIZE_T BufLen) | Cfps |
GetTcpIpPort(void) | Cfps |
GetTolerance(float &fUnterTolerance, float &fUeberTolerance) | Cfps |
GetUseCrcCheck(void) const | CTCPIPConnector | `[protected]`
GetVoltageSamples(float VoltageSample[640], unsigned int uiBegin=0, unsigned int uiLength=640) | Cfps |
initialize(void) | Cfps | `[virtual]`
CTCPIPConnector::initialize(const short TCPport, const char *pIPAddress) | CTCPIPConnector | `[virtual]`
InitModem(void) | Cfps |
IsConnected(void) const | CTCPIPConnector |
IsSamplingDone(bool &bDone) | Cfps |
m_bRcvRawData | CTCPIPConnector | `[protected]`
m_bRcvRawDataFinished | CTCPIPConnector | `[protected]`
m_oConvert | Cfps |
m_sRcvRawDataString | CTCPIPConnector | `[protected]`
MM enum Wert | Cfps |
MODEM enum Wert | Cfps |
MV enum Wert | Cfps |
NETZWERK enum Wert | Cfps |
PasswordLogin(char *szIpAddress, char *szPassword, unsigned int uiBasePort, unsigned int uiPortnumber) | Cfps |
ReadEepromData(ADDRESS_TYPE nAddress, unsigned int uiLength) | CTCPIPConnector |
ReadFpsEeprom(ADDRESS_TYPE nAddress, unsigned int uiLength) | Cfps | `[protected]`
ReadFpsProgram(ADDRESS_TYPE nAddress, unsigned int uiLength) | Cfps | `[protected]`
ReadFpsRam(ADDRESS_TYPE nAddress, unsigned int uiLength) | Cfps | `[protected]`
ReadInterpolatedSensor(SENSOR_TYPE &CurrentSensorValues) | Cfps |
ReadProfileFile(const std::string &sFilename) | Cfps |
ReadProfileFileConnectionType(const std::string &sFilename) | Cfps |
ReadProgramData(ADDRESS_TYPE nAddress, unsigned int uiLength) | CTCPIPConnector |
ReadRamData(ADDRESS_TYPE nAddress, unsigned int uiLength) | CTCPIPConnector |
ReadSensor(SENSOR_TYPE &CurrentSensorValues) | Cfps |
Receive(void *pData, long DataLen) | CTCPIPConnector | `[protected]`
ResetEx(void) | Cfps |
RS232 enum Wert | Cfps |
SaveTolerance(float fUnterTolerance, float fUeberTolerance) | Cfps |
SendReadEepromDataCnf(ADDRESS_TYPE nAddress, const std::vector< unsigned char > &aucData) | CTCPIPConnector |
SendReadProgramDataCnf(ADDRESS_TYPE nAddress, const std::vector< unsigned char > &aucData) | CTCPIPConnector |
SendReadRamDataCnf(ADDRESS_TYPE nAddress, const std::vector< unsigned char > &aucData) | CTCPIPConnector |
SendStatusInfo(ADDRESS_TYPE nAddress, unsigned int uiLength, std::vector< unsigned char > aucData) | CTCPIPConnector |
SendWriteEepromDataCnf(ADDRESS_TYPE nAddress, unsigned int uiLength) | CTCPIPConnector |
SendWriteProgramDataCnf(ADDRESS_TYPE nAddress, unsigned int uiLength) | CTCPIPConnector |
SendWriteRamDataCnf(ADDRESS_TYPE nAddress, unsigned int uiLength) | CTCPIPConnector |
SetBasePort(const unsigned int nBasePort) | Cfps |
SetCallnumber(char *pcNewCallnumber) | Cfps |
SetCallNumber(char *pcNewCallNumber) | Cfps |
SetCOMPort(CCOMConnector *pMsg) | CTCPIPConnector | `[inline]`
SetCurrentConnectionType(const VERBINDUNG eNewConnectionType) | Cfps |
SetModemConnectString(char *pcModemConnectString) | Cfps |
SetModemDialString(char *pcNewModemDialString) | Cfps |
SetModemDialTimeout(const unsigned int uiNewTimeoutValue) | Cfps |
SetModemInitString(char *pcNewModemInitString) | Cfps |
SetModemInitTimeout(const unsigned int uiNewTimeOut) | Cfps |
SetModemOkString(char *pcModemOkString) | Cfps |
SetOperatingState(int Flags) | Cfps |
SetRcvTimeOut(const DWORD dwNewTimeOut) | Cfps |
SetTcpIpAddress(char const *pcIpAddress) | Cfps |
SetTcpIpPort(unsigned int uiNewPort) | Cfps |
SetUseCrcCheck(const bool bUseCrc) | CTCPIPConnector | `[protected]`
SPEC enum Wert | Cfps |
StartSampling(void) | Cfps |
StoreData(const RECEIVED_TYPE Command, const ADDRESS_TYPE nAddress, const unsigned int uiLength, const std::vector< unsigned char > &aucData=std::vector< unsigned char >::vector()) | Cfps |
StoreStuetzArrayInFps(void) | Cfps |
terminate(void) | CTCPIPConnector |
VERBINDUNG enum Bezeichner | Cfps |
WaitForData(void) | Cfps | `[protected]`
WriteEepromData(ADDRESS_TYPE nAddress, const std::vector< unsigned char > &aucData) | CTCPIPConnector |
WriteFpsEeprom(ADDRESS_TYPE nAddress, unsigned int uiLength, std::vector< unsigned char > aucData) | Cfps | `[protected]`
WriteFpsProgram(ADDRESS_TYPE nAddress, unsigned int uiLength, std::vector< unsigned char > aucData) | Cfps | `[protected]`
WriteFpsRam(ADDRESS_TYPE nAddress, unsigned int uiLength, std::vector< unsigned char > aucData) | Cfps | `[protected]`
WriteProfileFile(std::string sFilename) | Cfps |
WriteProgramData(ADDRESS_TYPE nAddress, const std::vector< unsigned char > &aucData) | CTCPIPConnector |
WriteRamData(ADDRESS_TYPE nAddress, const std::vector< unsigned char > &aucData) | CTCPIPConnector |
WriteSensor(SENSOR_TYPE NewSensorValues) | Cfps |
~Cfps() | Cfps | `[virtual]`
~CTCPIPConnector() | CTCPIPConnector | `[virtual]`