Hauptseite | Klassenhierarchie | Alphabetische Liste | Auflistung der Klassen | Auflistung der Dateien | Klassen-Elemente | Datei-Elemente

# rcvbuffer.hpp Dateireferenz

## Klassen
class | CRcvBuffer
| handles the received data Mehr...
## Aufzählungen
enum | RECEIVED_TYPE { NONE, CONNECT, DISCONNECT, READ_EEPROM_REQ, READ_EEPROM_CNF, READ_PROGRAM_REQ, READ_PROGRAM_CNF, READ_RAM_REQ, READ_RAM_CNF, WRITE_EEPROM_REQ, WRITE_EEPROM_CNF, WRITE_PROGRAM_REQ, WRITE_PROGRAM_CNF, WRITE_RAM_REQ, WRITE_RAM_CNF, STATUS_INFORMATION }
| all possible received commands memory and memory types relatives to the memory on the fps controller Mehr...

## Dokumentation der Aufzählungstypen

enum RECEIVED_TYPE

  | Aufzählungswerte:
  NONE |
  CONNECT | no command
  DISCONNECT | connection established
  READ_EEPROM_REQ | connection broken
  READ_EEPROM_CNF | we want to read data from eeprom
  READ_PROGRAM_REQ | we get the requested eeprom data
  READ_PROGRAM_CNF | we want to read data from program memory
  READ_RAM_REQ | we get the requested data from program memory
  READ_RAM_CNF | we want to read data from ram
  WRITE_EEPROM_REQ | we get the requested data from ram
  WRITE_EEPROM_CNF | we want to write data into the eeprom
  WRITE_PROGRAM_REQ | indicates if the data were successfully written
  WRITE_PROGRAM_CNF | we want to write data into the program
  WRITE_RAM_REQ | indicates if the data were successfully written
  WRITE_RAM_CNF | we want to write data into the ram
  STATUS_INFORMATION | send by fps during startup and in case of an error